========== /dev/sdg ==========

smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Vendor:               HGST
Product:              HUH721010AL42C0
Revision:             A3Z4
Compliance:           SPC-4
User Capacity:        10,000,831,348,736 bytes [10.0 TB]
Logical block size:   4096 bytes
LU is fully provisioned
Rotation Rate:        7200 rpm
Form Factor:          3.5 inches
Logical Unit id:      0x5000cca26aba9678
Serial number:        2TK9M3ND
Device type:          disk
Transport protocol:   SAS (SPL-4)
Local Time is:        Mon Jul  6 05:33:51 2026 UTC
SMART support is:     Available - device has SMART capability.
SMART support is:     Enabled
Temperature Warning:  Enabled


----- SMART Health & Attributes -----
smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF READ SMART DATA SECTION ===
SMART Health Status: OK

Format status indicates no format since manufacture
Current Drive Temperature:     28 C
Drive Trip Temperature:        85 C

Accumulated power on time, hours:minutes 57669:32
Manufactured in week 17 of year 2018
Specified cycle count over device lifetime:  50000
Accumulated start-stop cycles:  23
Specified load-unload count over device lifetime:  600000
Accumulated load-unload cycles:  2410
Elements in grown defect list: 0


----- Extended SMART (error log, self-test log, device statistics) -----
smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Vendor:               HGST
Product:              HUH721010AL42C0
Revision:             A3Z4
Compliance:           SPC-4
User Capacity:        10,000,831,348,736 bytes [10.0 TB]
Logical block size:   4096 bytes
LU is fully provisioned
Rotation Rate:        7200 rpm
Form Factor:          3.5 inches
Logical Unit id:      0x5000cca26aba9678
Serial number:        2TK9M3ND
Device type:          disk
Transport protocol:   SAS (SPL-4)
Local Time is:        Mon Jul  6 05:33:51 2026 UTC
SMART support is:     Available - device has SMART capability.
SMART support is:     Enabled
Temperature Warning:  Enabled
Read Cache is:        Enabled
Writeback Cache is:   Disabled

=== START OF READ SMART DATA SECTION ===
SMART Health Status: OK

Format status indicates no format since manufacture
Current Drive Temperature:     28 C
Drive Trip Temperature:        85 C

Manufactured in week 17 of year 2018
Specified cycle count over device lifetime:  50000
Accumulated start-stop cycles:  23
Specified load-unload count over device lifetime:  600000
Accumulated load-unload cycles:  2410
Elements in grown defect list: 0

Vendor (Seagate Cache) information
  Blocks sent to initiator = 14247518900584448

Error counter log:
           Errors Corrected by           Total   Correction     Gigabytes    Total
               ECC          rereads/    errors   algorithm      processed    uncorrected
           fast | delayed   rewrites  corrected  invocations   [10^9 bytes]  errors
read:          0       48         0        48    9408464     581751.132           0
write:         0        0         0         0    2133227     393157.284           0
verify:        0      316         0       316      40794    3450287.331           0

Non-medium error count:        0

SMART Self-test log
Num  Test              Status                 segment  LifeTime  LBA_first_err [SK ASC ASQ]
     Description                              number   (hours)
# 1  Background short  Completed                   -   57669                 - [-   -    -]
# 2  Background short  Completed                   -   57618                 - [-   -    -]

Long (extended) Self-test duration: 72900 seconds [20.2 hours]

Background scan results log
  Status: scan is active
    Accumulated power on time, hours:minutes 57669:32 [3460172 minutes]
    Number of background scans performed: 344,  scan progress: 4.39%
    Number of background medium scans performed: 344

General statistics and performance log page:
  General access statistics and performance:
    Number of read commands: 1476205116
    Number of write commands: 849218303
    number of logical blocks received: 95985664944
    number of logical blocks transmitted: 142029084983
    read command processing intervals: 0
    write command processing intervals: 0
    weighted number of read commands plus write commands: 0
    weighted read command processing plus write command processing: 0
  Idle time:
    Idle time intervals: 3432793150
      in seconds: 171639657.500
      in hours: 47677.682

Protocol Specific port log page for SAS SSP
relative target port id = 1
  generation code = 2
  number of phys = 1
  phy identifier = 0
    attached device type: expander device
    attached reason: SMP phy control function
    reason: unknown
    negotiated logical link rate: phy enabled; 12 Gbps
    attached initiator port: ssp=0 stp=0 smp=0
    attached target port: ssp=0 stp=0 smp=1
    SAS address = 0x5000cca26aba9679
    attached SAS address = 0x500304802116027f
    attached phy identifier = 6
    Invalid DWORD count = 0
    Running disparity error count = 0
    Loss of DWORD synchronization count = 0
    Phy reset problem count = 0
relative target port id = 2
  generation code = 2
  number of phys = 1
  phy identifier = 1
    attached device type: no device attached
    attached reason: unknown
    reason: power on
    negotiated logical link rate: phy enabled; unknown
    attached initiator port: ssp=0 stp=0 smp=0
    attached target port: ssp=0 stp=0 smp=0
    SAS address = 0x5000cca26aba967a
    attached SAS address = 0x0
    attached phy identifier = 0
    Invalid DWORD count = 0
    Running disparity error count = 0
    Loss of DWORD synchronization count = 0
    Phy reset problem count = 0


