========== /dev/sdf ==========

smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Vendor:               NETAPP
Product:              X377_STATE10TA07
Revision:             NA00
Compliance:           SPC-4
User Capacity:        10,000,831,348,736 bytes [10.0 TB]
Logical block size:   512 bytes
Physical block size:  4096 bytes
LU is fully provisioned
Rotation Rate:        7200 rpm
Form Factor:          3.5 inches
Logical Unit id:      0x5000c500ca0a5843
Serial number:        ZA2D33ES
Device type:          disk
Transport protocol:   SAS (SPL-4)
Local Time is:        Mon Jul  6 05:33:49 2026 UTC
SMART support is:     Available - device has SMART capability.
SMART support is:     Enabled
Temperature Warning:  Enabled


----- SMART Health & Attributes -----
smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF READ SMART DATA SECTION ===
SMART Health Status: OK

Grown defects during certification = 0
Total blocks reassigned during format = 2
Total new blocks reassigned = 0
Power on minutes since format = 5831
Current Drive Temperature:     26 C
Drive Trip Temperature:        40 C

Accumulated power on time, hours:minutes 36360:44
Manufactured in week 15 of year 2020
Specified cycle count over device lifetime:  10000
Accumulated start-stop cycles:  133
Specified load-unload count over device lifetime:  300000
Accumulated load-unload cycles:  1550
Elements in grown defect list: 2


----- Extended SMART (error log, self-test log, device statistics) -----
smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.0-27-generic] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Vendor:               NETAPP
Product:              X377_STATE10TA07
Revision:             NA00
Compliance:           SPC-4
User Capacity:        10,000,831,348,736 bytes [10.0 TB]
Logical block size:   512 bytes
Physical block size:  4096 bytes
LU is fully provisioned
Rotation Rate:        7200 rpm
Form Factor:          3.5 inches
Logical Unit id:      0x5000c500ca0a5843
Serial number:        ZA2D33ES
Device type:          disk
Transport protocol:   SAS (SPL-4)
Local Time is:        Mon Jul  6 05:33:50 2026 UTC
SMART support is:     Available - device has SMART capability.
SMART support is:     Enabled
Temperature Warning:  Enabled
Read Cache is:        Enabled
Writeback Cache is:   Disabled

=== START OF READ SMART DATA SECTION ===
SMART Health Status: OK

Grown defects during certification = 0
Total blocks reassigned during format = 2
Total new blocks reassigned = 0
Power on minutes since format = 5831
Current Drive Temperature:     26 C
Drive Trip Temperature:        40 C

Manufactured in week 15 of year 2020
Specified cycle count over device lifetime:  10000
Accumulated start-stop cycles:  133
Specified load-unload count over device lifetime:  300000
Accumulated load-unload cycles:  1550
Elements in grown defect list: 2

Error counter log:
           Errors Corrected by           Total   Correction     Gigabytes    Total
               ECC          rereads/    errors   algorithm      processed    uncorrected
           fast | delayed   rewrites  corrected  invocations   [10^9 bytes]  errors
read:   2459169398        0         0  2459169398          0    2011974.306           0
write:         0        0         0         0          0      37100.051           0
verify: 1348352988        0         0  1348352988          0     113775.818           0

Non-medium error count:      388

SMART Self-test log
Num  Test              Status                 segment  LifeTime  LBA_first_err [SK ASC ASQ]
     Description                              number   (hours)
# 1  Background short  Completed                   -   36360                 - [-   -    -]
# 2  Background short  Completed                   -   36309                 - [-   -    -]

Long (extended) Self-test duration: 56880 seconds [15.8 hours]

Background scan results log
  Status: no scans active
    Accumulated power on time, hours:minutes 36360:44 [2181644 minutes]
    Number of background scans performed: 0,  scan progress: 0.00%
    Number of background medium scans performed: 0
Device does not support General statistics and performance logging

Protocol Specific port log page for SAS SSP
relative target port id = 1
  generation code = 2
  number of phys = 1
  phy identifier = 0
    attached device type: expander device
    attached reason: SMP phy control function
    reason: unknown
    negotiated logical link rate: phy enabled; 12 Gbps
    attached initiator port: ssp=0 stp=0 smp=0
    attached target port: ssp=0 stp=0 smp=1
    SAS address = 0x5000c500ca0a5841
    attached SAS address = 0x500304802116027f
    attached phy identifier = 5
    Invalid DWORD count = 0
    Running disparity error count = 0
    Loss of DWORD synchronization count = 7
    Phy reset problem count = 11
relative target port id = 2
  generation code = 2
  number of phys = 1
  phy identifier = 1
    attached device type: no device attached
    attached reason: unknown
    reason: unknown
    negotiated logical link rate: phy enabled; unknown
    attached initiator port: ssp=0 stp=0 smp=0
    attached target port: ssp=0 stp=0 smp=0
    SAS address = 0x5000c500ca0a5842
    attached SAS address = 0x0
    attached phy identifier = 0
    Invalid DWORD count = 0
    Running disparity error count = 0
    Loss of DWORD synchronization count = 0
    Phy reset problem count = 2


